# 3D Printing Summary

|  |  |
| --- | --- |
| **Metric** |  |
| Total Print Time (min) | 34 |
| Total Number of Components | 2 |
| Typical Total Mass (g) | 6.3 |
| Typical Number of Print Setups | 1 |

# 3D Printing Settings

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Print File Name** | **Qty** | **Total Print Time (hr:min)** | **Mass (g)** | **Infill (%)** | **Support(Y/N)** | **Layer Height/ Nozzle Diameter(mm)** | **Notes (orientation, special settings, etc)** |
| Top.stl | 1 | 0:22 | 3.8 | 20 | N | 0.2/0.4 | - |
| Bottom.stl | 1 | 0:16 | 2.5 | 20 | N | 0.2/0.4 | - Print in given orientation |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |

# Customization Options

The user can request different colours for the top and/or bottom enclosure.

# Post-Processing

Clean up any stringing and smooth any sharp edges. Can optionally use a marker or paint to make the labels more readable.

# Examples of Quality Prints:

